# See docs/devel/tracing.txt for syntax documentation.

# hw/misc/eccmemctl.c
ecc_mem_writel_mer(uint32_t val) "Write memory enable 0x%08x"
ecc_mem_writel_mdr(uint32_t val) "Write memory delay 0x%08x"
ecc_mem_writel_mfsr(uint32_t val) "Write memory fault status 0x%08x"
ecc_mem_writel_vcr(uint32_t val) "Write slot configuration 0x%08x"
ecc_mem_writel_dr(uint32_t val) "Write diagnostic 0x%08x"
ecc_mem_writel_ecr0(uint32_t val) "Write event count 1 0x%08x"
ecc_mem_writel_ecr1(uint32_t val) "Write event count 2 0x%08x"
ecc_mem_readl_mer(uint32_t ret) "Read memory enable 0x%08x"
ecc_mem_readl_mdr(uint32_t ret) "Read memory delay 0x%08x"
ecc_mem_readl_mfsr(uint32_t ret) "Read memory fault status 0x%08x"
ecc_mem_readl_vcr(uint32_t ret) "Read slot configuration 0x%08x"
ecc_mem_readl_mfar0(uint32_t ret) "Read memory fault address 0 0x%08x"
ecc_mem_readl_mfar1(uint32_t ret) "Read memory fault address 1 0x%08x"
ecc_mem_readl_dr(uint32_t ret) "Read diagnostic 0x%08x"
ecc_mem_readl_ecr0(uint32_t ret) "Read event count 1 0x%08x"
ecc_mem_readl_ecr1(uint32_t ret) "Read event count 2 0x%08x"
ecc_diag_mem_writeb(uint64_t addr, uint32_t val) "Write diagnostic %"PRId64" = 0x%02x"
ecc_diag_mem_readb(uint64_t addr, uint32_t ret) "Read diagnostic %"PRId64"= 0x%02x"

# hw/misc/slavio_misc.c
slavio_misc_update_irq_raise(void) "Raise IRQ"
slavio_misc_update_irq_lower(void) "Lower IRQ"
slavio_set_power_fail(int power_failing, uint8_t config) "Power fail: %d, config: %d"
slavio_cfg_mem_writeb(uint32_t val) "Write config 0x%02x"
slavio_cfg_mem_readb(uint32_t ret) "Read config 0x%02x"
slavio_diag_mem_writeb(uint32_t val) "Write diag 0x%02x"
slavio_diag_mem_readb(uint32_t ret) "Read diag 0x%02x"
slavio_mdm_mem_writeb(uint32_t val) "Write modem control 0x%02x"
slavio_mdm_mem_readb(uint32_t ret) "Read modem control 0x%02x"
slavio_aux1_mem_writeb(uint32_t val) "Write aux1 0x%02x"
slavio_aux1_mem_readb(uint32_t ret) "Read aux1 0x%02x"
slavio_aux2_mem_writeb(uint32_t val) "Write aux2 0x%02x"
slavio_aux2_mem_readb(uint32_t ret) "Read aux2 0x%02x"
apc_mem_writeb(uint32_t val) "Write power management 0x%02x"
apc_mem_readb(uint32_t ret) "Read power management 0x%02x"
slavio_sysctrl_mem_writel(uint32_t val) "Write system control 0x%08x"
slavio_sysctrl_mem_readl(uint32_t ret) "Read system control 0x%08x"
slavio_led_mem_writew(uint32_t val) "Write diagnostic LED 0x%04x"
slavio_led_mem_readw(uint32_t ret) "Read diagnostic LED 0x%04x"

# hw/misc/milkymist-hpdmc.c
milkymist_hpdmc_memory_read(uint32_t addr, uint32_t value) "addr=0x%08x value=0x%08x"
milkymist_hpdmc_memory_write(uint32_t addr, uint32_t value) "addr=0x%08x value=0x%08x"

# hw/misc/milkymist-pfpu.c
milkymist_pfpu_memory_read(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
milkymist_pfpu_memory_write(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
milkymist_pfpu_vectout(uint32_t a, uint32_t b, uint32_t dma_ptr) "a 0x%08x b 0x%08x dma_ptr 0x%08x"
milkymist_pfpu_pulse_irq(void) "Pulse IRQ"

# hw/misc/aspeed_scu.c
aspeed_scu_write(uint64_t offset, unsigned size, uint32_t data) "To 0x%" PRIx64 " of size %u: 0x%" PRIx32

# hw/misc/mps2_scc.c
mps2_scc_read(uint64_t offset, uint64_t data, unsigned size) "MPS2 SCC read: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u"
mps2_scc_write(uint64_t offset, uint64_t data, unsigned size) "MPS2 SCC write: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u"
mps2_scc_reset(void) "MPS2 SCC: reset"
mps2_scc_leds(char led7, char led6, char led5, char led4, char led3, char led2, char led1, char led0) "MPS2 SCC LEDs: %c%c%c%c%c%c%c%c"
mps2_scc_cfg_write(unsigned function, unsigned device, uint32_t value) "MPS2 SCC config write: function %d device %d data 0x%" PRIx32
mps2_scc_cfg_read(unsigned function, unsigned device, uint32_t value) "MPS2 SCC config read: function %d device %d data 0x%" PRIx32
