# See docs/devel/tracing.txt for syntax documentation.

# hw/i386/x86-iommu.c
x86_iommu_iec_notify(bool global, uint32_t index, uint32_t mask) "Notify IEC invalidation: global=%d index=%" PRIu32 " mask=%" PRIu32

# hw/i386/intel_iommu.c
vtd_inv_desc(const char *type, uint64_t hi, uint64_t lo) "invalidate desc type %s high 0x%"PRIx64" low 0x%"PRIx64
vtd_inv_desc_invalid(uint64_t hi, uint64_t lo) "invalid inv desc hi 0x%"PRIx64" lo 0x%"PRIx64
vtd_inv_desc_cc_domain(uint16_t domain) "context invalidate domain 0x%"PRIx16
vtd_inv_desc_cc_global(void) "context invalidate globally"
vtd_inv_desc_cc_device(uint8_t bus, uint8_t dev, uint8_t fn) "context invalidate device %02"PRIx8":%02"PRIx8".%02"PRIx8
vtd_inv_desc_cc_devices(uint16_t sid, uint16_t fmask) "context invalidate devices sid 0x%"PRIx16" fmask 0x%"PRIx16
vtd_inv_desc_cc_invalid(uint64_t hi, uint64_t lo) "invalid context-cache desc hi 0x%"PRIx64" lo 0x%"PRIx64
vtd_inv_desc_iotlb_global(void) "iotlb invalidate global"
vtd_inv_desc_iotlb_domain(uint16_t domain) "iotlb invalidate whole domain 0x%"PRIx16
vtd_inv_desc_iotlb_pages(uint16_t domain, uint64_t addr, uint8_t mask) "iotlb invalidate domain 0x%"PRIx16" addr 0x%"PRIx64" mask 0x%"PRIx8
vtd_inv_desc_iotlb_invalid(uint64_t hi, uint64_t lo) "invalid iotlb desc hi 0x%"PRIx64" lo 0x%"PRIx64
vtd_inv_desc_wait_sw(uint64_t addr, uint32_t data) "wait invalidate status write addr 0x%"PRIx64" data 0x%"PRIx32
vtd_inv_desc_wait_irq(const char *msg) "%s"
vtd_inv_desc_wait_invalid(uint64_t hi, uint64_t lo) "invalid wait desc hi 0x%"PRIx64" lo 0x%"PRIx64
vtd_inv_desc_wait_write_fail(uint64_t hi, uint64_t lo) "write fail for wait desc hi 0x%"PRIx64" lo 0x%"PRIx64
vtd_inv_desc_iec(uint32_t granularity, uint32_t index, uint32_t mask) "granularity 0x%"PRIx32" index 0x%"PRIx32" mask 0x%"PRIx32
vtd_inv_qi_enable(bool enable) "enabled %d"
vtd_inv_qi_setup(uint64_t addr, int size) "addr 0x%"PRIx64" size %d"
vtd_inv_qi_head(uint16_t head) "read head %d"
vtd_inv_qi_tail(uint16_t head) "write tail %d"
vtd_inv_qi_fetch(void) ""
vtd_context_cache_reset(void) ""
vtd_re_not_present(uint8_t bus) "Root entry bus %"PRIu8" not present"
vtd_re_invalid(uint64_t hi, uint64_t lo) "invalid root entry hi 0x%"PRIx64" lo 0x%"PRIx64
vtd_ce_not_present(uint8_t bus, uint8_t devfn) "Context entry bus %"PRIu8" devfn %"PRIu8" not present"
vtd_ce_invalid(uint64_t hi, uint64_t lo) "invalid context entry hi 0x%"PRIx64" lo 0x%"PRIx64
vtd_iotlb_page_hit(uint16_t sid, uint64_t addr, uint64_t slpte, uint16_t domain) "IOTLB page hit sid 0x%"PRIx16" iova 0x%"PRIx64" slpte 0x%"PRIx64" domain 0x%"PRIx16
vtd_iotlb_page_update(uint16_t sid, uint64_t addr, uint64_t slpte, uint16_t domain) "IOTLB page update sid 0x%"PRIx16" iova 0x%"PRIx64" slpte 0x%"PRIx64" domain 0x%"PRIx16
vtd_iotlb_cc_hit(uint8_t bus, uint8_t devfn, uint64_t high, uint64_t low, uint32_t gen) "IOTLB context hit bus 0x%"PRIx8" devfn 0x%"PRIx8" high 0x%"PRIx64" low 0x%"PRIx64" gen %"PRIu32
vtd_iotlb_cc_update(uint8_t bus, uint8_t devfn, uint64_t high, uint64_t low, uint32_t gen1, uint32_t gen2) "IOTLB context update bus 0x%"PRIx8" devfn 0x%"PRIx8" high 0x%"PRIx64" low 0x%"PRIx64" gen %"PRIu32" -> gen %"PRIu32
vtd_iotlb_reset(const char *reason) "IOTLB reset (reason: %s)"
vtd_fault_disabled(void) "Fault processing disabled for context entry"
vtd_replay_ce_valid(uint8_t bus, uint8_t dev, uint8_t fn, uint16_t domain, uint64_t hi, uint64_t lo) "replay valid context device %02"PRIx8":%02"PRIx8".%02"PRIx8" domain 0x%"PRIx16" hi 0x%"PRIx64" lo 0x%"PRIx64
vtd_replay_ce_invalid(uint8_t bus, uint8_t dev, uint8_t fn) "replay invalid context device %02"PRIx8":%02"PRIx8".%02"PRIx8
vtd_page_walk_level(uint64_t addr, uint32_t level, uint64_t start, uint64_t end) "walk (base=0x%"PRIx64", level=%"PRIu32") iova range 0x%"PRIx64" - 0x%"PRIx64
vtd_page_walk_one(uint32_t level, uint64_t iova, uint64_t gpa, uint64_t mask, int perm) "detected page level 0x%"PRIx32" iova 0x%"PRIx64" -> gpa 0x%"PRIx64" mask 0x%"PRIx64" perm %d"
vtd_page_walk_skip_read(uint64_t iova, uint64_t next) "Page walk skip iova 0x%"PRIx64" - 0x%"PRIx64" due to unable to read"
vtd_page_walk_skip_perm(uint64_t iova, uint64_t next) "Page walk skip iova 0x%"PRIx64" - 0x%"PRIx64" due to perm empty"
vtd_page_walk_skip_reserve(uint64_t iova, uint64_t next) "Page walk skip iova 0x%"PRIx64" - 0x%"PRIx64" due to rsrv set"
vtd_switch_address_space(uint8_t bus, uint8_t slot, uint8_t fn, bool on) "Device %02x:%02x.%x switching address space (iommu enabled=%d)"
vtd_as_unmap_whole(uint8_t bus, uint8_t slot, uint8_t fn, uint64_t iova, uint64_t size) "Device %02x:%02x.%x start 0x%"PRIx64" size 0x%"PRIx64
vtd_translate_pt(uint16_t sid, uint64_t addr) "source id 0x%"PRIu16", iova 0x%"PRIx64
vtd_pt_enable_fast_path(uint16_t sid, bool success) "sid 0x%"PRIu16" %d"
vtd_irq_generate(uint64_t addr, uint64_t data) "addr 0x%"PRIx64" data 0x%"PRIx64
vtd_reg_read(uint64_t addr, uint64_t size) "addr 0x%"PRIx64" size 0x%"PRIx64
vtd_reg_write(uint64_t addr, uint64_t size, uint64_t val) "addr 0x%"PRIx64" size 0x%"PRIx64" value 0x%"PRIx64
vtd_reg_dmar_root(uint64_t addr, bool extended) "addr 0x%"PRIx64" extended %d"
vtd_reg_ir_root(uint64_t addr, uint32_t size) "addr 0x%"PRIx64" size 0x%"PRIx32
vtd_reg_write_gcmd(uint32_t status, uint32_t val) "status 0x%"PRIx32" value 0x%"PRIx32
vtd_reg_write_fectl(uint32_t value) "value 0x%"PRIx32
vtd_reg_write_iectl(uint32_t value) "value 0x%"PRIx32
vtd_reg_ics_clear_ip(void) ""
vtd_dmar_translate(uint8_t bus, uint8_t slot, uint8_t func, uint64_t iova, uint64_t gpa, uint64_t mask) "dev %02x:%02x.%02x iova 0x%"PRIx64" -> gpa 0x%"PRIx64" mask 0x%"PRIx64
vtd_dmar_enable(bool en) "enable %d"
vtd_dmar_fault(uint16_t sid, int fault, uint64_t addr, bool is_write) "sid 0x%"PRIx16" fault %d addr 0x%"PRIx64" write %d"
vtd_ir_enable(bool en) "enable %d"
vtd_ir_irte_get(int index, uint64_t lo, uint64_t hi) "index %d low 0x%"PRIx64" high 0x%"PRIx64
vtd_ir_remap(int index, int tri, int vec, int deliver, uint32_t dest, int dest_mode) "index %d trigger %d vector %d deliver %d dest 0x%"PRIx32" mode %d"
vtd_ir_remap_type(const char *type) "%s"
vtd_ir_remap_msi(uint64_t addr, uint64_t data, uint64_t addr2, uint64_t data2) "(addr 0x%"PRIx64", data 0x%"PRIx64") -> (addr 0x%"PRIx64", data 0x%"PRIx64")"
vtd_ir_remap_msi_req(uint64_t addr, uint64_t data) "addr 0x%"PRIx64" data 0x%"PRIx64
vtd_fsts_ppf(bool set) "FSTS PPF bit set to %d"
vtd_fsts_clear_ip(void) ""
vtd_frr_new(int index, uint64_t hi, uint64_t lo) "index %d high 0x%"PRIx64" low 0x%"PRIx64
vtd_err(const char *str) "%s"
vtd_err_dmar_iova_overflow(uint64_t iova) "iova 0x%"PRIx64
vtd_err_dmar_slpte_read_error(uint64_t iova, int level) "iova 0x%"PRIx64" level %d"
vtd_err_dmar_slpte_perm_error(uint64_t iova, int level, uint64_t slpte, bool is_write) "iova 0x%"PRIx64" level %d slpte 0x%"PRIx64" write %d"
vtd_err_dmar_slpte_resv_error(uint64_t iova, int level, uint64_t slpte) "iova 0x%"PRIx64" level %d slpte 0x%"PRIx64
vtd_err_dmar_translate(uint8_t bus, uint8_t slot, uint8_t func, uint64_t iova) "dev %02x:%02x.%02x iova 0x%"PRIx64
vtd_warn_invalid_qi_tail(uint16_t tail) "tail 0x%"PRIx16
vtd_err_qi_disable(uint16_t head, uint16_t tail, int type) "head 0x%"PRIx16" tail 0x%"PRIx16" last_desc_type %d"
vtd_err_qi_tail(uint16_t tail, uint16_t size) "tail 0x%"PRIx16" size 0x%"PRIx16
vtd_err_irte(int index, uint64_t lo, uint64_t hi) "index %d low 0x%"PRIx64" high 0x%"PRIx64
vtd_err_irte_sid(int index, uint16_t req, uint16_t target) "index %d SVT_ALL sid 0x%"PRIx16" (should be: 0x%"PRIx16")"
vtd_err_irte_sid_bus(int index, uint8_t bus, uint8_t min, uint8_t max) "index %d SVT_BUS bus 0x%"PRIx8" (should be: 0x%"PRIx8"-0x%"PRIx8")"
vtd_err_irte_svt(int index, int type) "index %d SVT type %d"
vtd_err_ir_msi_invalid(uint16_t sid, uint64_t addr, uint64_t data) "sid 0x%"PRIx16" addr 0x%"PRIx64" data 0x%"PRIx64
vtd_warn_ir_vector(uint16_t sid, int index, int vec, int target) "sid 0x%"PRIx16" index %d vec %d (should be: %d)"
vtd_warn_ir_trigger(uint16_t sid, int index, int trig, int target) "sid 0x%"PRIx16" index %d trigger %d (should be: %d)"

# hw/i386/amd_iommu.c
amdvi_evntlog_fail(uint64_t addr, uint32_t head) "error: fail to write at addr 0x%"PRIx64" +  offset 0x%"PRIx32
amdvi_cache_update(uint16_t domid, uint8_t bus, uint8_t slot, uint8_t func, uint64_t gpa, uint64_t txaddr) " update iotlb domid 0x%"PRIx16" devid: %02x:%02x.%x gpa 0x%"PRIx64" hpa 0x%"PRIx64
amdvi_completion_wait_fail(uint64_t addr) "error: fail to write at address 0x%"PRIx64
amdvi_mmio_write(const char *reg, uint64_t addr, unsigned size, uint64_t val, uint64_t offset) "%s write addr 0x%"PRIx64", size %u, val 0x%"PRIx64", offset 0x%"PRIx64
amdvi_mmio_read(const char *reg, uint64_t addr, unsigned size, uint64_t offset) "%s read addr 0x%"PRIx64", size %u offset 0x%"PRIx64
amdvi_mmio_read_invalid(int max, uint64_t addr, unsigned size) "error: addr outside region (max 0x%x): read addr 0x%" PRIx64 ", size %u"
amdvi_command_error(uint64_t status) "error: Executing commands with command buffer disabled 0x%"PRIx64
amdvi_command_read_fail(uint64_t addr, uint32_t head) "error: fail to access memory at 0x%"PRIx64" + 0x%"PRIx32
amdvi_command_exec(uint32_t head, uint32_t tail, uint64_t buf) "command buffer head at 0x%"PRIx32" command buffer tail at 0x%"PRIx32" command buffer base at 0x%"PRIx64
amdvi_unhandled_command(uint8_t type) "unhandled command 0x%"PRIx8
amdvi_intr_inval(void) "Interrupt table invalidated"
amdvi_iotlb_inval(void) "IOTLB pages invalidated"
amdvi_prefetch_pages(void) "Pre-fetch of AMD-Vi pages requested"
amdvi_pages_inval(uint16_t domid) "AMD-Vi pages for domain 0x%"PRIx16 " invalidated"
amdvi_all_inval(void) "Invalidation of all AMD-Vi cache requested "
amdvi_ppr_exec(void) "Execution of PPR queue requested "
amdvi_devtab_inval(uint8_t bus, uint8_t slot, uint8_t func) "device table entry for devid: %02x:%02x.%x invalidated"
amdvi_completion_wait(uint64_t addr, uint64_t data) "completion wait requested with store address 0x%"PRIx64" and store data 0x%"PRIx64
amdvi_control_status(uint64_t val) "MMIO_STATUS state 0x%"PRIx64
amdvi_iotlb_reset(void) "IOTLB exceed size limit - reset "
amdvi_dte_get_fail(uint64_t addr, uint32_t offset) "error: failed to access Device Entry devtab 0x%"PRIx64" offset 0x%"PRIx32
amdvi_invalid_dte(uint64_t addr) "PTE entry at 0x%"PRIx64" is invalid "
amdvi_get_pte_hwerror(uint64_t addr) "hardware error eccessing PTE at addr 0x%"PRIx64
amdvi_mode_invalid(uint8_t level, uint64_t addr)"error: translation level 0x%"PRIx8" translating addr 0x%"PRIx64
amdvi_page_fault(uint64_t addr) "error: page fault accessing guest physical address 0x%"PRIx64
amdvi_iotlb_hit(uint8_t bus, uint8_t slot, uint8_t func, uint64_t addr, uint64_t txaddr) "hit iotlb devid %02x:%02x.%x gpa 0x%"PRIx64" hpa 0x%"PRIx64
amdvi_translation_result(uint8_t bus, uint8_t slot, uint8_t func, uint64_t addr, uint64_t txaddr) "devid: %02x:%02x.%x gpa 0x%"PRIx64" hpa 0x%"PRIx64
