# See docs/devel/tracing.txt for syntax documentation.

# hw/timer/slavio_timer.c
slavio_timer_get_out(uint64_t limit, uint32_t counthigh, uint32_t count) "limit 0x%"PRIx64" count 0x%x0x%08x"
slavio_timer_irq(uint32_t counthigh, uint32_t count) "callback: count 0x%x0x%08x"
slavio_timer_mem_readl_invalid(uint64_t addr) "invalid read address 0x%"PRIx64
slavio_timer_mem_readl(uint64_t addr, uint32_t ret) "read 0x%"PRIx64" = 0x%08x"
slavio_timer_mem_writel(uint64_t addr, uint32_t val) "write 0x%"PRIx64" = 0x%08x"
slavio_timer_mem_writel_limit(unsigned int timer_index, uint64_t count) "processor %d user timer set to 0x%016"PRIx64
slavio_timer_mem_writel_counter_invalid(void) "not user timer"
slavio_timer_mem_writel_status_start(unsigned int timer_index) "processor %d user timer started"
slavio_timer_mem_writel_status_stop(unsigned int timer_index) "processor %d user timer stopped"
slavio_timer_mem_writel_mode_user(unsigned int timer_index) "processor %d changed from counter to user timer"
slavio_timer_mem_writel_mode_counter(unsigned int timer_index) "processor %d changed from user timer to counter"
slavio_timer_mem_writel_mode_invalid(void) "not system timer"
slavio_timer_mem_writel_invalid(uint64_t addr) "invalid write address 0x%"PRIx64

# hw/timer/grlib_gptimer.c
grlib_gptimer_enable(int id, uint32_t count) "timer:%d set count 0x%x and run"
grlib_gptimer_disabled(int id, uint32_t config) "timer:%d Timer disable config 0x%x"
grlib_gptimer_restart(int id, uint32_t reload) "timer:%d reload val: 0x%x"
grlib_gptimer_set_scaler(uint32_t scaler, uint32_t freq) "scaler:0x%x freq: 0x%x"
grlib_gptimer_hit(int id) "timer:%d HIT"
grlib_gptimer_readl(int id, uint64_t addr, uint32_t val) "timer:%d addr 0x%"PRIx64" 0x%x"
grlib_gptimer_writel(int id, uint64_t addr, uint32_t val) "timer:%d addr 0x%"PRIx64" 0x%x"

# hw/timer/lm32_timer.c
lm32_timer_memory_write(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
lm32_timer_memory_read(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
lm32_timer_hit(void) "timer hit"
lm32_timer_irq_state(int level) "irq state %d"

# hw/timer/milkymist-sysctl.c
milkymist_sysctl_memory_read(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
milkymist_sysctl_memory_write(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
milkymist_sysctl_icap_write(uint32_t value) "value 0x%08x"
milkymist_sysctl_start_timer0(void) "Start timer0"
milkymist_sysctl_stop_timer0(void) "Stop timer0"
milkymist_sysctl_start_timer1(void) "Start timer1"
milkymist_sysctl_stop_timer1(void) "Stop timer1"
milkymist_sysctl_pulse_irq_timer0(void) "Pulse IRQ Timer0"
milkymist_sysctl_pulse_irq_timer1(void) "Pulse IRQ Timer1"

# hw/timer/aspeed_timer.c
aspeed_timer_ctrl_enable(uint8_t i, bool enable) "Timer %" PRIu8 ": %d"
aspeed_timer_ctrl_external_clock(uint8_t i, bool enable) "Timer %" PRIu8 ": %d"
aspeed_timer_ctrl_overflow_interrupt(uint8_t i, bool enable) "Timer %" PRIu8 ": %d"
aspeed_timer_ctrl_pulse_enable(uint8_t i, bool enable) "Timer %" PRIu8 ": %d"
aspeed_timer_set_ctrl2(uint32_t value) "Value: 0x%" PRIx32
aspeed_timer_set_value(int timer, int reg, uint32_t value) "Timer %d register %d: 0x%" PRIx32
aspeed_timer_read(uint64_t offset, unsigned size, uint64_t value) "From 0x%" PRIx64 ": of size %u: 0x%" PRIx64

# hw/timer/armv7m_systick.c
systick_reload(void) "systick reload"
systick_timer_tick(void) "systick reload"
systick_read(uint64_t addr, uint32_t value, unsigned size) "systick read addr 0x%" PRIx64 " data 0x%" PRIx32 " size %u"
systick_write(uint64_t addr, uint32_t value, unsigned size) "systick write addr 0x%" PRIx64 " data 0x%" PRIx32 " size %u"

# hw/char/cmsdk_apb_timer.c
cmsdk_apb_timer_read(uint64_t offset, uint64_t data, unsigned size) "CMSDK APB timer read: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u"
cmsdk_apb_timer_write(uint64_t offset, uint64_t data, unsigned size) "CMSDK APB timer write: offset 0x%" PRIx64 " data 0x%" PRIx64 " size %u"
cmsdk_apb_timer_reset(void) "CMSDK APB timer: reset"
