QA output created by 083
=== Check disconnect before neg1 ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect after neg1 ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect 8 neg1 ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect 16 neg1 ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect before export ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect after export ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect 4 export ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect 12 export ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect 16 export ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect before neg2 ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect after neg2 ===

read failed: Input/output error

=== Check disconnect 8 neg2 ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect 10 neg2 ===

can't open device nbd+tcp://127.0.0.1:PORT/foo

=== Check disconnect before request ===

read failed: Input/output error

=== Check disconnect after request ===

read failed: Input/output error

=== Check disconnect before reply ===

read failed: Input/output error

=== Check disconnect after reply ===

read failed: Input/output error

=== Check disconnect 4 reply ===

Unexpected end-of-file before all bytes were read
read failed: Input/output error

=== Check disconnect 8 reply ===

Unexpected end-of-file before all bytes were read
read failed: Input/output error

=== Check disconnect before data ===

read failed: Input/output error

=== Check disconnect after data ===

read 512/512 bytes at offset 0
512 bytes, X ops; XX:XX:XX.X (XXX YYY/sec and XXX ops/sec)

=== Check disconnect before neg-classic ===

can't open device nbd+tcp://127.0.0.1:PORT/

=== Check disconnect 8 neg-classic ===

can't open device nbd+tcp://127.0.0.1:PORT/

=== Check disconnect 16 neg-classic ===

can't open device nbd+tcp://127.0.0.1:PORT/

=== Check disconnect 24 neg-classic ===

can't open device nbd+tcp://127.0.0.1:PORT/

=== Check disconnect 28 neg-classic ===

can't open device nbd+tcp://127.0.0.1:PORT/

=== Check disconnect after neg-classic ===

read failed: Input/output error

=== Check disconnect before neg1 ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect after neg1 ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect 8 neg1 ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect 16 neg1 ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect before export ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect after export ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect 4 export ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect 12 export ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect 16 export ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect before neg2 ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect after neg2 ===

read failed: Input/output error

=== Check disconnect 8 neg2 ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect 10 neg2 ===

can't open device nbd+unix:///foo?socket=TEST_DIR/nbd.sock

=== Check disconnect before request ===

read failed: Input/output error

=== Check disconnect after request ===

read failed: Input/output error

=== Check disconnect before reply ===

read failed: Input/output error

=== Check disconnect after reply ===

read failed: Input/output error

=== Check disconnect 4 reply ===

Unexpected end-of-file before all bytes were read
read failed: Input/output error

=== Check disconnect 8 reply ===

Unexpected end-of-file before all bytes were read
read failed: Input/output error

=== Check disconnect before data ===

read failed: Input/output error

=== Check disconnect after data ===

read 512/512 bytes at offset 0
512 bytes, X ops; XX:XX:XX.X (XXX YYY/sec and XXX ops/sec)

=== Check disconnect before neg-classic ===

can't open device nbd+unix:///?socket=TEST_DIR/nbd.sock

=== Check disconnect 8 neg-classic ===

can't open device nbd+unix:///?socket=TEST_DIR/nbd.sock

=== Check disconnect 16 neg-classic ===

can't open device nbd+unix:///?socket=TEST_DIR/nbd.sock

=== Check disconnect 24 neg-classic ===

can't open device nbd+unix:///?socket=TEST_DIR/nbd.sock

=== Check disconnect 28 neg-classic ===

can't open device nbd+unix:///?socket=TEST_DIR/nbd.sock

=== Check disconnect after neg-classic ===

read failed: Input/output error

*** done
